Country/Region

- United States
- ASEAN Region
- Australia
- 中国 - China
- France
- Deutschland - Germany
- India
- Italia - Italy
- 日本 - Japan
- 대한민국 - Korea
- Россия - Russia
- España - Spain
- 台灣 - Taiwan
- United Kingdom

Contact Us
|
Country/Region
United States

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

## Related Documentation

- Configuring Routing in the Core Network for VPLS in the JunosE BGP and MPLS Configuration Guide

# network area

#### Syntax

[ no ] network ipNet maskWildCard area { areaId | areaIdInt }

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Defines the interfaces on which OSPF runs and the area ID for those interfaces. The no version deletes OSPF interfaces, ranges, and areas.

| Note: Before you issue this command, you must first configure one or more interfaces with an IP address that is within the range specified by ipNet. Create address ranges that do not overlap; you can attach only the same range of interfaces to a single area.

#### Options

- ipNet—Network number
- maskWildCard—Wild-card mask for the network number
- areaId—OSPF area ID in IP address format
- areaIdInt—OSPF area ID as a decimal value, in the range 0–4294967295

#### Mode

Router Configuration

## Related Documentation

- Configuring Routing in the Core Network for VPLS in the JunosE BGP and MPLS Configuration Guide

#### Published: 2010-10-19

Help
|
My Account
|
Log Out