# Monitoring DHCP Packet Capture Settings

#### Purpose

Display the configuration for per-interface DHCP packet logging.

#### Action

To display configuration information about the DHCP packet capture feature:

    host1#show ip dhcp-capture

          Dhcp Capture Configuration
          --------------------------
    Router    Interface   Type    Priority
    -------   ---------   -----   --------
    default   ip3/1       Rx/Tx   low/low
    default   ip5/1       Rx      high

#### Meaning

Table 119 lists the show ip dhcp-capture command output fields.

Table 119: show ip dhcp-capture Output Fields

Field Name | Field Description
--- | ---
Router | Router name
Interface | Interface whose DHCP packets are logged
Type | Packet type to be logged, Rx (received), Tx (transmitted), or Rx/Tx (all)
Priority | Priority assigned to logged packets, low or high

#### Related Documentation

- show ip dhcp-capture