Country/Region

- United States
- ASEAN Region
- Australia
- 中国 - China
- France
- Deutschland - Germany
- India
- Italia - Italy
- 日本 - Japan
- 대한민국 - Korea
- Россия - Russia
- España - Spain
- 台灣 - Taiwan
- United Kingdom

Contact Us
|
Country/Region
United States

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

# ospf bandwidth

#### Syntax

[ no ] ospf bandwidth

#### Release Information

Command introduced in JunosE Release 10.3.0.

#### Description

Directs the router to use the bandwidth configured on an OSPF interface for OSPF interface cost calculation. If you configure the bandwidth and then issue the no ospf bandwidth command, the router ignores the cost that is calculated using the configured bandwidth. The no version disables the use of the bandwidth for OSPF interface cost calculation.

#### Mode

Router Configuration

#### Published: 2010-10-19

Help
|
My Account
|
Log Out