# Monitoring the Policy Configuration of Frame Relay Subinterfaces

#### Purpose

Display information about a subinterface’s Frame Relay policy lists.

#### Action

To display information about Frame Relay policy lists:

    host1#show frame-relay subinterface
    Frame relay sub-interface SERIAL5/0:1/1.1, status is up
    Number of sub-interface down transitions is 0
    Time since last status change 03:04:59
    No baseline has been set
      In bytes: 660                    Out bytes: 660
      In frames: 5                     Out frames: 5
      In errors: 0                     Out errors: 0
      In discards: 0                   Out discards: 0
      In unknown protos: 0
    Frame relay policy output frOutputPolicy
      classifier-group frGroupA entry 1
         5 packets, 640 bytes
         mark-de 1
    Frame relay sub-interface SERIAL5/1:1/1.1, status is up
    Number of sub-interface down transitions is 0
    Time since last status change 03:05:09
    No baseline has been set
      In bytes: 660                    Out bytes: 660
      In frames: 5                     Out frames: 5
      In errors: 0                     Out errors: 0
      In discards: 0                   Out discards: 0
      In unknown protos: 0
    Frame relay policy input frInputPolicy
      classifier-group frMatchDeSet entry 1
          5 packets, 660 bytes
          color red

#### Meaning

Table 35 lists the show frame-relay subinterface command output fields.

Table 35: show frame-relay subinterface Output Fields

Field Name | Field Description
--- | ---
Frame Relay policy | Type and name of the VLAN policy
mark-de | DE bit value
color | Color applied to packet flow for queuing: green, yellow, or red
classifier-group | Name of the classifier control list used by the policy
filter | Filter policy action
forward | Forward policy action
traffic class | Traffic class in the policy list
user-packet-class | User packet class in the policy list

#### Related Documentation

- show frame-relay subinterface