Country/Region

- United States
- ASEAN Region
- Australia
- 中国 - China
- France
- Deutschland - Germany
- India
- Italia - Italy
- 日本 - Japan
- 대한민국 - Korea
- Россия - Russia
- España - Spain
- 台灣 - Taiwan
- United Kingdom

Contact Us
|
Country/Region
United States

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

# tunnel mpls diff-serv phb-id

#### Syntax

tunnel mpls diff-serv phb-id { private privateId | standard standardId } [ exp-bits expBits ]

no tunnel mpls diff-serv phb-id { private privateId | standard standardId }

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Specifies the PHB supported by a signaled tunnel.

For E-LSPs, this command also maps the PHB to the specified EXP bits bitValue. You can repeat the command for up to eight PHB mappings.

For L-LSPs, the exp-bits keyword is not used. If you repeat the command, the most recent command overwrites the previous command.

The no version removes the mapping association.

#### Options

- privateId—Number, in the range 0–4095, designating the private PHB identifier
- standardId—Number, in the range 0–63, designating the standard identifier using the DSCP bits
- expBits—Number, in the range 0–7, designating the EXP bits

#### Mode

Interface Configuration, Tunnel Profile Configuration

#### Published: 2010-10-19

Help
|
My Account
|
Log Out