# traffic-class

#### Syntax

In Classifier Group Configuration mode:

[ no ] [ suspend ] traffic-class trafficClassName1

In Global Configuration and Traffic Class Group Configuration modes:

[ no ] traffic-class trafficClassName2

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

In Classifier Group Configuration mode, specifies a traffic class in a policy list for policy management. The no version removes a traffic class from a policy list; the suspend version temporarily suspends the policy rule; the no suspend version resumes application of a suspended rule.

| Note: This command replaces the Policy List Configuration version of the traffic-class command, which may be removed completely in a future release.

In Global Configuration mode, configures a traffic class in the E Series router. In Traffic Class Group Configuration mode, specifies a traffic class that belongs to the traffic-class group. The no version deletes the traffic class.

#### Options

- trafficClassName1—Name of the traffic class; up to 40 characters
- trafficClassName2—Name of the traffic class; up to 31 characters

#### Mode

Classifier Group Configuration, Global Configuration, Traffic Class Group Configuration

#### Related Documentation

- Configuring Traffic Classes That Define Service Levels
- Configuring Traffic-Class Groups That Define Service Levels
- Policy Rule Precedence