# Monitoring the Configuration of VRRP Tracked Objects

#### Purpose

Display details of objects tracked by various VRIDs.

#### Action

To display the details of objects tracked using VRIDs.

    host1#show ip vrrp tracked-objects
    Interface           Vrid       Priority   Object        Type       State   Decrement
    ----------------    -------    --------   ------        --------   -----   ---------
    FastEthernet3/0     1          100        ERX_Bangalore IP-route   Up      12
    FastEthernet3/0     1          100        ERX_Bangalore IP-route   Up      15
    FastEthernet3/0     1          100        ERX_Bangalore IP-route   Up      10
    FastEthernet3/0     2          100        ERX_Bangalore IP-route   Up      10
    FastEthernet3/0     3          100        ERX_Bangalore IP-route   Up      12
    FastEthernet3/0     3          100        ERX_Bangalore IP-route   Up      15

#### Meaning

Table 28 lists the show ip vrrp tracked-objects command output fields.

Table 28: show ip vrrp tracked-objects Output Fields

Field Name | Field Description
--- | ---
Interface | Name of the Interface. Fast Ethernet, Gigabit Ethernet, or 10-Gigabit Ethernet interface specifier.
Vrid | VRRP router instance configured on the interface
Priority | Priority of the VRRP router. If the priority value is 255, then the VRRP router is the master.
Object | Name of the object being tracked
Type | Type of object being tracked
State | State of the object
Decrement | Value by which the priority is decremented or restored following an object state change

#### Related Documentation

- Changing the Object Priority