Country/Region

- United States
- ASEAN Region
- Australia
- 中国 - China
- France
- Deutschland - Germany
- India
- Italia - Italy
- 日本 - Japan
- 대한민국 - Korea
- Россия - Russia
- España - Spain
- 台灣 - Taiwan
- United Kingdom

Contact Us
|
Country/Region
United States

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

# sscc address

#### Syntax

sscc { primary | secondary | tertiary } address ipAddress [ port portNumber ]

no sscc { primary | secondary | tertiary } address [ ipAddress [ port portNumber ] ]

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Configures the SRC client (formerly SSCC) with the IP addresses of the SRC servers and the ports on which the servers listen for activity. The no version removes the specified server (primary, secondary, or tertiary) from the list of SRC servers.

#### Options

- primary—Primary SRC server
- secondary—Secondary SRC server
- tertiary—Tertiary SRC server
- ipAddress—IP address of an SRC server
- portNumber—SRC server port number on which the server listens for activity; default port is 3288

#### Mode

Global Configuration

#### Published: 2010-10-19

Help
|
My Account
|
Log Out