Country/Region

- United States
- ASEAN Region
- Australia
- 中国 - China
- France
- Deutschland - Germany
- India
- Italia - Italy
- 日本 - Japan
- 대한민국 - Korea
- Россия - Russia
- España - Spain
- 台灣 - Taiwan
- United Kingdom

Contact Us
|
Country/Region
United States

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

## Related Documentation

- Configuring QoS for Tunnel-Server Ports for L2TP LNS Sessions

# tunnel-server

#### Syntax

[ no ] tunnel-server interfaceSpecifier

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Specifies the location of a dedicated or shared tunnel-server port on a module and accesses Tunnel Server Configuration mode, which enables you to provision the maximum number of tunnel-service interfaces to be used on the tunnel-server port. The default version restores the default configuration. On dedicated tunnel-server ports, the default configuration is the maximum number of tunnel-service interfaces that the tunnel-service module supports. On shared tunnel-server ports, the default configuration is zero tunnel-service interfaces provisioned. The no version unprovisions the tunnel-server port by reducing the number of provisioned tunnel-service interfaces to zero.

#### Options

- interfaceSpecifier—Particular interface; format varies according to interface type; see Interface Types and Specifiers; port number specified must have the tunnel-server port assigned to it

#### Mode

Global Configuration

## Related Documentation

- Configuring QoS for Tunnel-Server Ports for L2TP LNS Sessions

#### Published: 2010-10-19

Help
|
My Account
|
Log Out