# show redundancy line-card

#### Syntax

show redundancy line-card [ slot slotNum ] [ filter ]

#### Release Information

Command introduced before JunosE Release 7.1.0.

slot keyword and slotNum variable added in JunosE Release 11.3.0.

#### Description

Displays redundancy information specific to line modules, including supported redundancy modes and high availability status for a line module installed in a particular slot. If you enter this command without the slot keyword, redundancy details for all line modules on a router are displayed.

#### Options

- slotNum—Number of the slot in which the line module resides in the router; for the E120 router, a number in the range 0–5; for the E320 router, a number in the range 0–5 or 11–16
- filter—See Filtering show Commands

#### Mode

Privileged Exec