Country/Region

- United States
- ASEAN Region
- Australia
- 中国 - China
- France
- Deutschland - Germany
- India
- Italia - Italy
- 日本 - Japan
- 대한민국 - Korea
- Россия - Russia
- España - Spain
- 台灣 - Taiwan
- United Kingdom

Contact Us
|
Country/Region
United States

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

## Related Documentation

- Integrating the HRR Scheduler and SAR Scheduler
- Configuring Default Integrated Mode for ATM Interface
- Configuring Low-Latency Mode for Per-Port Queuing on ATM Interfaces
- Configuring Low-CDV Mode for Per-Port Queuing on ATM Interfaces
- Disabling Per-Port Queuing on ATM Interfaces

# qos-mode-port

#### Syntax

[ no ] qos-mode-port [ low-cdv | low-latency ]

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Configures an ATM port for per-port queuing. The no version restores the default integrated mode, removing per-port queuing from the ATM port; in this state, shaping done by the SAR is controlled by ATM.

#### Options

- low-cdv—HRR scheduler and SAR scheduler operate in concert. The SAR runs with more buffering than in low-latency mode, shaping rates are driven by QoS profiles, VC backpressure is disabled, and lenient port backpressure is enabled.
- low-latency—Shaping done by the SAR is controlled by QoS. The HRR scheduler controls the traffic rate. The SAR runs with minimal buffering, VC backpressure is disabled, and aggressive port backpressure is enabled. This is the behavior enforced if you do not specify an option.

#### Mode

Interface Configuration

## Related Documentation

- Integrating the HRR Scheduler and SAR Scheduler
- Configuring Default Integrated Mode for ATM Interface
- Configuring Low-Latency Mode for Per-Port Queuing on ATM Interfaces
- Configuring Low-CDV Mode for Per-Port Queuing on ATM Interfaces
- Disabling Per-Port Queuing on ATM Interfaces

#### Published: 2010-10-19

Help
|
My Account
|
Log Out