# Configuring Dynamic IPSec Subscribers

This chapter describes how to securely terminate IPSec remote access subscribers. These subscribers can reside on different VPNs and the router can support many VPNs simultaneously. It contains the following sections:

- Overview
- Platform Considerations
- References
- Creating an IPSec Tunnel Profile
- Configuring IPSec Tunnel Profiles
- Defining IKE Policy Rules for IPSec Tunnels
- Monitoring IPSec Tunnel Profiles