# LM-10 Line Module

> Module label | ES2 10G LM
> Number of ports | Not applicable
> Software release | First supported: 8.0.0
> Description | 198 W maximum Acts as frame forwarding engines for the physical interfaces Processes up to 10 Gb of data traffic Pairs with ES2–S2 10GE PR IOA and ES2–S1 GE-8 IOA In a SRP-100 configuration, it must be installed in a turbo slot only (slot 2 or slot 4) If you install the line module in a slot other than slot 2 or slot 4, it will be disabled If you install the LM-10 module next to a configured line module that is already installed in slot 3 or slot 5, the LM-10 module will be disabled If you install a line module in slot 3 or slot 5 next to a previously installed LM-10 module, the non-LM-10 module will be disabled In a SRP-120 and SRP-320 configuration, it can be installed in any slot
> Type | TFA ASIC
> Capability | Supports a line rate of 128–byte frames on IOAs The 100–Gbps switch fabric allocates 3.4 Gbps of overall bandwidth to each regular line module slot and 10 Gbps of overall bandwidth to each of the turbo slots (slot 2 and slot 4). The 120–Gbps and 320–Gbps switch fabrics allocate 10 Gbps of overall bandwidth to each line module slot. See JunosE System Basics Configuration Guide, Chapter 6, Managing Modules for more information.
> Software features | Not applicable
> Line module compatibility | Not applicable
> SRP module compatibility | SRP-100 SRP-120 SRP-320
> Line module redundancy compatibility | Yes (Redundancy IOA must be installed in either slot 0 or slot 11) Can only back up another ES2 10G LM
> Port redundancy support | Not applicable
> Cables and connectors | Not applicable
> LEDs | When lit, LED indicates: OK (green)—Self-test passed FAIL (red)—Failure detected ONLINE (green)—Online with no alarms or errors REDUN (green)—Redundant card available
> Alarms, errors, and events | See Monitoring Modules in JunosE System Basics Configuration Guide, Chapter 6, Managing Modules.