Country/Region

- United States
- ASEAN Region
- Australia
- 中国 - China
- France
- Deutschland - Germany
- India
- Italia - Italy
- 日本 - Japan
- 대한민국 - Korea
- Россия - Russia
- España - Spain
- 台灣 - Taiwan
- United Kingdom

Contact Us
|
Country/Region
United States

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

# profile vlan override bulk-config

#### Syntax

To configure an override for a single-tagged VLAN ID:

profile vlan override bulk-config bulkConfigName vlan vlanIdValue overrideProfileName

To configure an override for a double-tagged S-VLAN ID:

profile vlan override bulk-config bulkConfigName svlan s-vlanIdValue
{ vlanIdValue | any } overrideProfileName

To remove the profile override assignment:

no profile vlan override bulk-config bulkConfigName { svlan s-vlanId | vlan }
{ vlanId | any }

#### Release Information

Command introduced in JunosE Release 7.1.0.
bulk-config keyword and bulkConfigName variable added in JunosE Release 7.3.0.

#### Description

Assigns an overriding profile to a single-tagged VLAN ID or double-tagged S-VLAN ID that exists within a VLAN subrange previously configured with the vlan bulk-config command. The profile vlan override bulk-config command enables you to assign a special profile for the subscribers associated with a specific DSLAM. After the overriding profile is assigned, it is used instead of the previously assigned base profile to create any VLAN dynamic subinterface columns over the specified VLAN ID or double-tagged S-VLAN ID. The no version removes the overriding profile assignment for the VLAN ID or double-tagged S-VLAN ID and restores the original base profile assignment.

#### Options

- bulkConfigName—Name of the VLAN range; string of up to 80 characters
- s-vlanIdValue—S-VLAN ID number, in the range 0–4095
- vlanIdValue—VLAN ID number, in the range 0–4095
- overrideProfileName—Name of the profile for which you want to assign an override
- any—Specifies the VLAN ID as a wildcard

#### Mode

Interface Configuration

#### Published: 2010-10-19

Help
|
My Account
|
Log Out