Country/Region

- United States
- ASEAN Region
- Australia
- 中国 - China
- France
- Deutschland - Germany
- India
- Italia - Italy
- 日本 - Japan
- 대한민국 - Korea
- Россия - Russia
- España - Spain
- 台灣 - Taiwan
- United Kingdom

Contact Us
|
Country/Region
United States

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

## Related Documentation

- Per-Packet Queuing on the SAR Scheduler Overview
- Guidelines for Configuring QoS over ATM
- atm vp-tunnel
- interface atm
- qos-mode-port

# Configuring Default Integrated Mode for ATM Interface

In the default integrated mode, the SAR scheduler is the dominant scheduler, and it backpressures the first-stage (HRR) scheduler per VC. Each VC buffers only a few hundred bytes.

Figure 1 shows the default integrated mode.

Figure 1: Default Integrated Mode

To configure default integrated mode:

1. From the desired port, set the QoS port mode to default integrated mode.
   host1(config)#interface atm 2/0 host1(config-if)#no qos-mode-port

   | Tip: For ATM interfaces on ERX7xx models, ERX14xx models, and the ERX310 router, you must specify port 0.

2. Specify the VP shaping rate.
   host1(config-if)#atm vp-tunnel 0 2000

   | Tip: Configuring an ATM VP tunnel sets a shaping rate in the SAR scheduler. Before configuring an ATM VP tunnel, there must be no PVCs with the same VPI that you are about to configure. Before using the atm vp-tunnel command, remove any PVCs from the configuration. You can reconfigure the PVCs after configuring the shapeless VP tunnel.

3. Specify the shaping rate for the ATM subinterface.
   host1(config-if)#interface atm 2/0.5 host1(config-subif)#atm-pvc 5 0 5 aal5snap 768

## Related Documentation

- Per-Packet Queuing on the SAR Scheduler Overview
- Guidelines for Configuring QoS over ATM
- atm vp-tunnel
- interface atm
- qos-mode-port

#### Published: 2010-09-22

Help
|
My Account
|
Log Out