Country/Region

- United States
- ASEAN Region
- Australia
- 中国 - China
- France
- Deutschland - Germany
- India
- Italia - Italy
- 日本 - Japan
- 대한민국 - Korea
- Россия - Russia
- España - Spain
- 台灣 - Taiwan
- United Kingdom

Contact Us
|
Country/Region
United States

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

# set dhcp relay giaddr-selects-interface

#### Syntax

[ no ] set dhcp relay giaddr-selects-interface

#### Release Information

Command introduced in JunosE Release 8.0.0.

#### Description

Configures DHCP relay to use information in the giaddr in the DHCP ACK packets that are generated by the server and destined for the DHCP client. The DHCP server uses this information to determine the primary interface that is used to optionally build dynamic subscriber interfaces.

The no version restores the default that builds dynamic subscriber interfaces on the IP interface on which DHCP client discover packets are received.

#### Mode

Global Configuration

#### Published: 2010-10-19

Help
|
My Account
|
Log Out