Country/Region

- United States
- ASEAN Region
- Australia
- 中国 - China
- France
- Deutschland - Germany
- India
- Italia - Italy
- 日本 - Japan
- 대한민국 - Korea
- Россия - Russia
- España - Spain
- 台灣 - Taiwan
- United Kingdom

Contact Us
|
Country/Region
United States

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

## Related Documentation

- Monitoring QoS Parameter Instances

# show qos-parameter

#### Syntax

To display settings for a specific parameter instance with references:

show qos-parameter [ qosParameterInstanceName ] references [ brief | full ] [ filter ]

To display references globally:

show qos-parameter [ qosParameterInstanceName ] references global
[ qosParameterInstanceName ] [ brief | full ] [ filter ]

To display references for interfaces:

show qos-parameter [ qosParameterInstanceName ] references [ interface interfaceType interfaceSpecifier [ atmVpi | s-vlanIdValue ] ] [ explicit ] [ brief | full ]
[ filter ]

To display references for L2TP sessions:

show qos-parameter [ qosParameterInstanceName ] references lt2p session sessionName [ explicit ] [ filter ]

#### Release Information

Command introduced in JunosE Release 7.1.0.
full keyword added in JunosE Release 7.2.0.

#### Description

Displays QoS parameter instance settings for QoS clients.

#### Options

- qosParameterInstanceName—Name of the parameter instance
- references—Displays interfaces that reference this parameter instance
- global—Displays information about global parameter instances
- interfaceType—Interface type; see Interface Types and Specifiers
- interfaceSpecifier—Particular interface; format varies according to interface type; see Interface Types and Specifiers
- atmVpi—Virtual path identifier of this PVC; number in the range 0–255
- s-vlanIdValue—S-VLAN ID number in the range 0–4095
- sessionName —Name of the L2TP session
- brief—Displays information in a condensed format
- full—Displays information in expanded format
- explicit—Displays parameter instances only on the specified interface and not parameter instances stacked above the interface
- filter—See Filtering show Commands

#### Mode

Privileged Exec, User Exec

## Related Documentation

- Monitoring QoS Parameter Instances

#### Published: 2010-10-19

Help
|
My Account
|
Log Out