# Monitoring Active Subscriber Sessions with Service Manager

#### Purpose

Display information about active subscriber sessions on your router.

#### Action

To display summary information for all active subscriber sessions:

    host1# show service-management subscriber-session brief
                                 Subscriber Sessions
                                 -------------------
                                                                                 Service
         Name          Interface       Id   Owner/Id      State    Non-volatile  Sessions
    ----------------   --------------  --   ---------     ------   ------------  --------
    CLIENT1@ISP.COM    ip192.168.0.3   1    AAA 4194326   Active   False         1
    CLIENT2@ISP.COM    ip192.168.0.7   2    AAA 4194327   Active   False         1
    CLIENT3@ISP.COM    ip192.168.0.4   3    AAA 4194328   Active   False         1
    CLIENT4@ISP.COM    ip192.168.0.5   4    AAA 4194329   Active   False         1
    CLIENT5@ISP.COM    ip192.168.0.6   5    AAA 4194330   Active   False         1
    CLIENT6@ISP.COM    ip192.168.0.8   6    AAA 4194331   Active   False         1
    CLIENT7@ISP.COM    ip192.168.0.1   7    AAA 4194332   Active   False         1
    CLIENT8@ISP.COM    ip192.168.0.9   8    AAA 4194333   Active   False         1
    CLIENT9@ISP.COM    ip192.168.0.2   9    AAA 4194334   Active   False         1
    CLIENT10@ISP.COM   ip192.168.0.10  10   AAA 4194335   Active   False         1

To display information for that particular subscriber with the subscriber name:

    host1# show service-management subscriber-session client1@isp.com interface ip 192.168.0.1
    User Name: CLIENT1@ISP.COM, Interface: ip 192.168.0.1
     Id: 1
     Owner: AAA 4194326
     Non-volatile: False
     State: Active
     ServiceSessions:
             Name             mutex   Owner/Id      State                Operation
    -----------------------   -----   -----------   ------------------   ---------
    tiered(2000000,3000000)           AAA 4194326   ConfigApplySuccess   Activate
             Name             Non-volatile
    -----------------------   ------------
    tiered(2000000,3000000)   False

To display information for that particular subscriber with the service session:

    host1# show service-management subscriber-session client1@isp.COM interface ip 192.168.0.1 service-session tiered
    User Name: client1@isp.COM, Interface: ip192.168.0.1
    Service : tiered(2000000,3000000)
     Non-volatile : False
     Owner : AAA 41943236
     State : Config ApplySuccess
     Activate : True
     Statistics Type : time-based and volume-based
     Statistics Complete : False
     Poll Interval : 0
     Poll Expire : 0
     Activate Time : THU MAR 02 01:21:26 2006
     Time : 0
     Time Expire : 0
     Volume MBytes: 2
     Volume Expire MBytes : 1
     Input Bytes : 594
     Output Bytes : 1196
     Input Packets : 1
     Output Packets : 2

To display information for a particular subscriber using the subscriber ID:

    host1#show service-management subscriber-session 20

    User Name: CLIENT50@ISP.COM, Interface: ip192.168.100.33
     Id: 20
     Owner/Id: CLI
     Non-volatile: True
     State: Active
     ServiceSessions:
          Name            mutex   Owner   State                 Operation
    -------------------   -----   -----   -------------------   ---------
    internet(5000,8000)      12   CLI     Config ApplySuccess   Activate

          Name            Non-volatile
    ------------------    ------------
    internet(5000,8000)   True

#### Meaning

Table 164 lists the show service-management subscriber-session command output fields.

Table 164: show service-management subscriber-session Output Fields

Field Name | Field Description
--- | ---
Name | Name of the subscriber or name of the service session
Interface | Type and IP address of the subscriber’s interface
Id | ID number of the subscriber session
mutex | Index number of the mutex group to which the service session belongs
Owner/Id | Method used to activate the subscriber session (CLI, AAA) and ID number generated by the owner (Acct-Session-ID for AAA)
State | Status of the subscriber session (active or inactive), or status of the service session
Non-volatile | Indicates whether the service session is stored in NVS; RADIUS-based service sessions are not stored in NVS
Service Sessions | Number of service sessions currently active for this subscriber
Operation | Last operation that Service Manager performed
Service | Name of the service, with parameter values in parentheses
Activate | Indicates whether the last operation was activate (True) or deactivate (False)
Statistics Type | Type of statistics collected; none, time, or volume-time
Statistics Complete | Whether statistics have been successfully collected; True or False
Poll Interval | Interval, in seconds, that interim statistics reports are sent
Poll Expire | Number of seconds until the next statistics report is sent
Activate Time | Day, date, and time when the service session was activated
Time | Time threshold value set by service session profile or RADIUS VSA
Time Expire | Time left until the threshold expires; this value starts as the time threshold value and is decremented as time passes
Volume | Volume threshold value set by service session profile or RADIUS VSA
Volume Expire | Volume left until the threshold is exceeded; this value starts as the volume threshold value and is decremented as the service statistics measure volume
Input Bytes | Current value of input bytes that the statistics configuration is measuring
Output Bytes | Current value of output bytes that the statistics configuration is measuring
Input Packets | Current value of input packets that the statistics configuration is measuring
Output Packets | Current value of output packets that the statistics configuration is measuring

#### Related Documentation

- show service-management subscriber-session