Country/Region

- United States
- ASEAN Region
- Australia
- 中国 - China
- France
- Deutschland - Germany
- India
- Italia - Italy
- 日本 - Japan
- 대한민국 - Korea
- Россия - Russia
- España - Spain
- 台灣 - Taiwan
- United Kingdom

Contact Us
|
Country/Region
United States

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

# suspicious-control-flow-detection protocol low-threshold

#### Syntax

suspicious-control-flow-detection protocol protocolValue
low-threshold lowThresholdValue

no suspicious-control-flow-detection protocol protocolValue low-threshold

#### Release Information

Command introduced in JunosE Release 7.3.0.

#### Description

Sets the low threshold rate at which a suspicious flow becomes no longer suspicious for a specific protocol. The no version restores the default for a protocol, which is a protocol-dependent non-zero numeric value.

#### Options

- protocolValue—Name of the protocol
- lowThresholdValue—Threshold value in packets per second; 0 or a number in the range 1–32767; a value of zero means that a suspicious flow cannot change to the nonsuspicious state via a threshold; a flow can only become nonsuspicious via a backoff time; if the low threshold value is zero and the backoff time is zero, the flow can only be considered nonsuspicious if the rate (in packets per second) goes to zero

#### Mode

Global Configuration

#### Published: 2010-10-19

Help
|
My Account
|
Log Out