# dsu mode

#### Syntax

dsu mode { 0 | 2 }

no dsu mode

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Sets the DSU mode for the lines. The no version clears the dsu mode. If you issue this command, be sure to issue the dsu bandwidth and scramble commands. Similarly, if you issue the no version, be sure to issue the no versions of thedsu bandwidth and scramble commands; otherwise, the interface may drop packets unexpectedly.

#### Options

- 0—Sets digital Link mode
- 2—Sets Larscom mode

#### Mode

Controller Configuration