Country/Region

- United States
- ASEAN Region
- Australia
- 中国 - China
- France
- Deutschland - Germany
- India
- Italia - Italy
- 日本 - Japan
- 대한민국 - Korea
- Россия - Russia
- España - Spain
- 台灣 - Taiwan
- United Kingdom

Contact Us
|
Country/Region
United States

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

# vlan bulk-config shutdown

#### Syntax

To shut down or reenable the specified bulk configuration or a specific VLAN range:

[ no ] vlan bulk-config bulkConfigName shutdown

[ no ] vlan bulk-config bulkConfigName shutdown vlan-range vlanIdStart vlanIdEnd

To shut down or reenable VLAN ranges containing double-tagged S-VLAN IDs or based on agent-circuit-identifier information:

[ no ] vlan bulk-config bulkConfigName shutdown svlan-range s-vlanIdStart s-vlanIdEnd
{ vlanIdStart vlanIdEnd | any | agent-circuit-identifier }

#### Release Information

Command introduced in JunosE Release 7.3.0.

#### Description

Administratively disables (shuts down) the specified bulk configuration, or a specified VLAN range or subrange. When you shut down a specified bulk configuration, all VLAN ranges, including those based on double-tagged S-VLAN IDs or agent-circuit-identifier information, are disabled. The no version reenables the specified bulk configuration, the specified VLAN range, or the specified subranges; this is the default condition.

#### Options

- bulkConfigName—Name of the VLAN range; string of up to 80 characters
- vlanIdStart—Starting VLAN ID of the VLAN subrange you are configuring
- vlanIdEnd—Ending VLAN ID of the VLAN subrange you are configuring
- s-vlanIdStart—Starting S-VLAN ID of the S-VLAN subrange you are configuring
- s-vlanIdEnd—Ending S-VLAN ID of the S-VLAN subrange you are configuring
- any—Specifies the VLAN ID as a wildcard
- agent-circuit-identifier—Specifies a VLAN range that is based on agent-circuit-identifier information

#### Mode

Interface Configuration

#### Published: 2010-10-19

Help
|
My Account
|
Log Out