# Example: Configuring Frame Relay over MPLS

The script provided in this section is one way to configure Frame Relay services over MPLS. Explanation notes are provided within the script. You must change the script for your specific configuration.

The topology example shown in Figure 121 further explains the configuration script.

| Note: The route interface command is used toward the end of the configuration script. You can substitute the mpls-relay command, depending on the tunneling method best for your environment.

Figure 121: Sample Frame Relay over MPLS Configuration

    hostname "host 1"
    exception protocol ftp anonymous null
    !--------------------------------------------------------------------------
    !Configure CT3 interfaces in slot 4 for Frame Relay.
    !--------------------------------------------------------------------------
    !
    controller t3 4/0
     no shutdown
     clock source internal module
     cablelength 5
     t1 1 clock source internal module
     t1 1/1 timeslots 1-24 speed 64
     t1 2 clock source internal module
     t1 2/1 timeslots 1-24 speed 64
    !
    controller t3 4/1
     no shutdown
     clock source internal module
     cablelength 5
     t1 1 clock source internal module
     t1 1/1 timeslots 1-24 speed 64
     t1 2 clock source internal module
     t1 2/1 timeslots 1-24 speed 64
    !--------------------------------------------------------------------------
    !Create virtual router default.
    !--------------------------------------------------------------------------
    virtual-router default
    interface loopback 0
      ip address 222.9.1.1 255.255.255.255
    !--------------------------------------------------------------------------
    !Configure Frame Relay interfaces.
    !--------------------------------------------------------------------------
    interface serial 4/0:1/1
     encapsulation frame-relay ietf
    interface serial 4/0:1/1.1
    frame-relay interface-dlci 17 ietf
    !
    interface serial 4/0:2/1
     encapsulation frame-relay ietf
    interface serial 4/0:2/1.1
    frame-relay interface-dlci 12 ietf
    !
    interface serial 4/1:1/1
     encapsulation frame-relay ietf
     frame-relay intf-type dce
    interface serial 4/1:1/1.1
    frame-relay interface-dlci 17 ietf
    !
    interface serial 4/1:2/1
     encapsulation frame-relay ietf
     frame-relay intf-type dce
    interface serial 4/1:2/1.1
    frame-relay interface-dlci 12 ietf
    !--------------------------------------------------------------------------
    !Create virtual router two. Configure MPLS.
    !--------------------------------------------------------------------------
    virtual-router two

    mpls
    mpls ldp tar send list 222.9.1.3

    interface loopback 0
      ip address 222.9.1.2 255.255.255.255
      ip router isis

    interface atm 2/0
     atm clock inter mod
    interface atm 2/0.1
     atm pvc 1 1 11 aal5snap
     ip address 10.10.11.2 255.255.255.0
     ip router isis
     mpls
     mpls ldp
    router isis
     net 47.0005.80FF.F800.0000.0000.0004.0000.F209.0202.00
     mpls traffic-eng router-id loopback 0
     mpls traffic-eng level-1
     metric-style wide
    !--------------------------------------------------------------------------
    !Create virtual router three. Configure MPLS.
    !--------------------------------------------------------------------------
    virtual-router three

    mpls
    mpls ldp tar send list 222.9.1.2

    interface loopback 0
      ip address 222.9.1.3 255.255.255.255
      ip router isis

    interface atm 2/0.2
     atm pvc 2 1 12 aal5snap
     ip address 10.10.12.3 255.255.255.0
     ip router isis
     mpls
     mpls ldp

    router isis
     net 47.0005.80FF.F800.0000.0000.0004.0000.F209.0303.00
     mpls traffic-eng router-id loopback 0
     mpls traffic-eng level-1
     metric-style wide
    !--------------------------------------------------------------------------
    !Create virtual router four.
    !--------------------------------------------------------------------------
    virtual-router four

    interface loopback 0
      ip address 222.9.1.4 255.255.255.255

    !--------------------------------------------------------------------------
    !Create virtual router five. Configure MPLS.
    !--------------------------------------------------------------------------

    virtual-router five

    mpls

    interface loopback 0
      ip address 222.9.1.5 255.255.255.255
      ip router isis

    interface atm 2/1.1
     atm pvc 1 1 11 aal5snap
     ip address 10.10.11.5 255.255.255.0
     ip router isis
     mpls
     mpls ldp

    interface atm 2/1.2
     atm pvc 2 1 12 aal5snap
     ip address 10.10.12.5 255.255.255.0
     ip router isis
     mpls
     mpls ldp

    router isis
     net 47.0005.80FF.F800.0000.0000.0004.0000.F209.0505.00
     mpls traffic-eng router-id loopback 0
     mpls traffic-eng level-1
     metric-style wide
     !--------------------------------------------------------------------------
     !Create MPLS tunnel from VR three to VR two. Route Frame Relay traffic via MPLS tunnel.
     !--------------------------------------------------------------------------
     vir three

     interface tunnel mpls:3
     tunnel destination 222.9.1.2

     interface serial 4/1:2/1.1
     route interface tunnel mpls:3 45

     vir two

     interface tunnel mpls:2
     tunnel destination 222.9.1.3

     int ser 4/1:1/1.1
     route interface tunnel mpls:2 45