Country/Region

- United States
- ASEAN Region
- Australia
- 中国 - China
- France
- Deutschland - Germany
- India
- Italia - Italy
- 日本 - Japan
- 대한민국 - Korea
- Россия - Russia
- España - Spain
- 台灣 - Taiwan
- United Kingdom

Contact Us
|
Country/Region
United States

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

## Related Documentation

- Configuring Interface Supersets for QoS

# restricted

#### Syntax

[ no ] restricted interface restrictedInterfaceType interfaceSpecifier [ atmVpi | s-vlanIdValue ]

#### Release Information

Command introduced in JunosE Release 9.2.0.

#### Description

Configures an interface superset as restricted to a particular ATM-VPI or S-VLAN ID. The no version deletes the restriction for the interface superset.

#### Options

- restrictedInterfaceType—One of the following restricted interface types: atm-vp, fastEthernet, gigabitEthernet, svlan, tenGigabitEthernet
- interfaceSpecifier—Particular interface; format varies according to interface type; see Interface Types and Specifiers
- atmVpi—Virtual path identifier of this PVC; number in the range 0–255
- s-vlanIdValue—S-VLAN ID number in the range 0–4095

#### Mode

QoS Interface Superset Configuration

## Related Documentation

- Configuring Interface Supersets for QoS

#### Published: 2010-10-19

Help
|
My Account
|
Log Out