Country/Region

- United States
- ASEAN Region
- Australia
- 中国 - China
- France
- Deutschland - Germany
- India
- Italia - Italy
- 日本 - Japan
- 대한민국 - Korea
- Россия - Russia
- España - Spain
- 台灣 - Taiwan
- United Kingdom

Contact Us
|
Country/Region
United States

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

# member-interface

#### Syntax

[ no ] member-interface interfaceType interfaceSpecifier

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Adds a member interface, also known as a bundle member, to an MLPPP bundle, an MLFR bundle, or an IEEE 802.3ad link aggregation group (LAG) bundle. The no version removes the specified member interface from the bundle.

#### Options

- interfaceType—One of the following interface types listed in Interface Types and Specifiers
  - serial (MLFR bundle or MLPPP bundle)
  - pos (MLFR bundle only)
  - fastEthernet (IEEE 802.3ad LAG bundle only)
  - gigabitEthernet (IEEE 802.3ad LAG bundle only)
- interfaceSpecifier—Particular interface; format varies according to interface type; see Interface Types and Specifiers

#### Mode

Interface Configuration, Subinterface Configuration

#### Published: 2010-10-04

Help
|
My Account
|
Log Out