# ipEngine

#### Description

IP chassis manager

#### Emergency

None

#### Alert

None

#### Critical

None

#### Error

Failure in operations such as adding, removing, or deleting interfaces or distributing routing tables to line modules

#### Warning Log

Errors such as attempting to configure something that is not supported on a module, or routing table memory is approaching 80 percent full

#### Notice Log

Something unexpected happened; for example, an interface was deleted twice or, internal to the software, connections between IC and SRP were deleted twice

#### Info

Completion status of a user command (for example: “ IS command succeeded” )

#### Debug

An engine or agent that corresponds to a virtual router is added or deleted; an interface is added or deleted

#### Filter

None