Country/Region

- United States
- ASEAN Region
- Australia
- 中国 - China
- France
- Deutschland - Germany
- India
- Italia - Italy
- 日本 - Japan
- 대한민국 - Korea
- Россия - Russia
- España - Spain
- 台灣 - Taiwan
- United Kingdom

Contact Us
|
Country/Region
United States

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

## Related Documentation

- Supported Interface Types for QoS Profiles
- Configuring a QoS Profile

# QoS Profile Overview

You create an interface hierarchy for QoS by configuring a QoS profile that specifies queue profiles, drop profiles, statistics profiles, and scheduler profiles in combination with interface types. A QoS profile specifies the queue, drop statistics gathering, and scheduler configuration for a subtree of the interface hierarchy. The QoS profile controls the way scheduler nodes, queues, and shadow nodes are bound to the interfaces above its attachment point in the interface hierarchy.

You can attach a QoS profile to the interface at the base of the subtree hierarchy, an ATM VP, or an S-VLAN. For example, a QoS profile attached to an ATM port specifies queuing attributes for interfaces of all types that are stacked over the port.

## Related Documentation

- Supported Interface Types for QoS Profiles
- Configuring a QoS Profile

#### Published: 2010-09-22

Help
|
My Account
|
Log Out