# Monitoring MLPPP

Use the commands in this section to display information about MLPPP interfaces.

You can set a statistics baseline for MLPPP serial (member link) or bundle (multilink) interfaces using the baseline ppp command. Use the delta keyword with the show commands described below to display statistics with the baseline values subtracted.

After you configure multilink PPP, you can use the show ppp interface commands to display configuration and statistics information about MLPPP and MLPPP fragmentation and reassembly.

You can use the output filtering feature of the show command to include or exclude lines of output based on a text string you specify. For details, see section show Commands in JunosE System Basics Configuration Guide.

| Note: The E120 and E320 routers output for monitor and show commands is identical to output from other E Series routers, except that the E120 and E320 routers output also includes information about the adapter identifier in the interface specifier (slot/adapter/port).

baseline ppp interface

- Use to set a statistics baseline for PPP interfaces—including MLPPP interfaces, either individual serial (member link) interfaces or multilink (bundle) interfaces.
- Use only the serial or mlppp keywords.
- For serial interfaces, specify the interface location in the format slot/port:channel/subchannel for CT3 modules.
- For MLPPP interfaces, specify the interface location as the name of the MLPPP bundle.
- The router implements the baseline by reading and storing the statistics at the time the baseline is set and then subtracting this baseline whenever baseline-relative statistics are retrieved.
- When baselining is requested, the time since the last baseline was set is displayed in hours:minutes:seconds or days/hours format. If a baseline was not set, the following message is displayed instead:

      No baseline has been set

- Use the optional delta keyword with MLPPP show commands to specify that baselined statistics are to be shown.
- Example
  host1#baseline ppp interface serial 2/0:1/1
- There is no no version.
- See baseline ppp interface.

Sample Display Without Baseline

The following command displays PPP interface (including MLPPP interface) statistics without baselining:

    host1#show ppp interface statistics

    PPP interface serial 2/0:4/1 is up
    No baseline has been set
    Interface statistics              in                  out
       packets                        0                   0
       octets                         572                 684
       errors                         0                   0
       discards                       0                   0
    PPP interface serial 2/0:5/1 is up
    No baseline has been set
    Interface statistics              in                  out
       packets                        0                   0
       octets                         572                 684
       errors                         0                   0
       discards                       0                   0
    PPP interface serial 2/1:4/1 is up
    No baseline has been set
    Interface statistics              in                  out
       packets                        0                   0
       octets                         572                 684
       errors                         0                   0
       discards                       0                   0
    PPP interface serial 2/1:5/1 is up
    No baseline has been set
    Interface statistics              in                  out
       packets                        0                   0
       octets                         572                 684
       errors                         0                   0
       discards                       0                   0
    4 ppp interfaces found

    PPP interface mlppp group1 is up
    PPP multilink member-interface serial 2/0:1/1 is up
    No baseline has been set
    Interface statistics              in                  out
       packets                        0                   0
       octets                         608                 716
       errors                         0                   0
       discards                       0                   0
    PPP multilink member-interface serial 2/0:2/1 is up
    No baseline has been set
    Interface statistics              in                  out
       packets                        0                   0
       octets                         608                 716
       errors                         0                   0
       discards                       0                   0
    PPP multilink member-interface serial 2/0:3/1 is up
    No baseline has been set
    Interface statistics              in                  out
       packets                        0                   0
       octets                         596                 704
       errors                         0                   0
       discards                       0                   0

    PPP interface mlppp group2 is up
    PPP multilink member-interface serial 2/1:1/1 is up
    No baseline has been set
    Interface statistics              in                  out
       packets                        0                   0
       octets                         628                 740
       errors                         0                   0
       discards                       0                   0
    PPP multilink member-interface serial 2/1:2/1 is up
    No baseline has been set
    Interface statistics              in                  out
       packets                        0                   0
       octets                         628                 740
       errors                         0                   0
       discards                       0                   0
    PPP multilink member-interface serial 2/1:3/1 is up
    No baseline has been set
    Interface statistics              in                  out
       packets                        0                   0
       octets                         616                 728
       errors                         0                   0
       discards                       0                   0
    2 mlppp interfaces found

Sample Display with Baseline

The following command displays PPP interface (including MLPPP interface) statistics with baselining:

    host1#show ppp interface statistics delta

    PPP interface serial 2/0:4/1 is up
    Time since last baseline 00:00:35
    Interface statistics              in                  out
       packets                        0                   0
       octets                         75                  82
       errors                         0                   0
       discards                       0                   0
    PPP interface serial 2/0:5/1 is up
    Time since last baseline 00:00:37
    Interface statistics              in                  out
       packets                        0                   0
       octets                         87                  90
       errors                         0                   0
       discards                       0                   0
    PPP interface serial 2/1:4/1 is up
    Time since last baseline 00:00:39
    Interface statistics              in                  out
       packets                        0                   0
       octets                         101                 112
       errors                         0                   0
       discards                       0                   0
    PPP interface serial 2/1:5/1 is up
    Time since last baseline 00:00:43
    Interface statistics              in                  out
       packets                        0                   0
       octets                         94                  99
       errors                         0                   0
       discards                       0                   0
    4 ppp interfaces found
    PPP interface mlppp group1 is up
    PPP multilink member-interface serial 2/0:1/1 is up
    Time since last baseline 00:00:17
    Interface statistics              in                  out
       packets                        0                   0
       octets                         28                  26
       errors                         0                   0
       discards                       0                   0
    PPP multilink member-interface serial 2/0:2/1 is up
    Time since last baseline 00:10:22

    Interface statistics              in                  out
       packets                        0                   0
       octets                         102                 104
       errors                         0                   0
       discards                       0                   0
    PPP multilink member-interface serial 2/0:3/1 is up
    Time since last baseline 00:00:19
    Interface statistics              in                  out
       packets                        0                   0
       octets                         112                 126
       errors                         0                   0
       discards                       0                   0

    PPP interface mlppp group2 is up
    PPP multilink member-interface serial 2/1:1/1 is up
    Time since last baseline 00:00:23
    Interface statistics              in                  out
       packets                        0                   0
       octets                         125                 132
       errors                         0                   0
       discards                       0                   0
    PPP multilink member-interface serial 2/1:2/1 is up
    Time since last baseline 00:00:25
    Interface statistics              in                  out
       packets                        0                   0
       octets                         135                 138
       errors                         0                   0
       discards                       0                   0
    PPP multilink member-interface serial 2/1:3/1 is up
    Time since last baseline 00:00:30
    Interface statistics              in                  out
       packets                        0                   0
       octets                         125                 132
       errors                         0                   0
       discards                       0                   0
    2 mlppp interfaces found

show ppp interface mlppp

- Use to display information about MLPPP interfaces.
- You can display a great variety of information with this complex command. See the show ppp interface command in Configuring Point-to-Point Protocol, for more detailed information about the display options.
- Use the show ppp interface command to display information about all PPP interfaces, including MLPPP interfaces.
- Field descriptions
  - PPP interface mlppp—Name and administrative status (up or down) for an MLPPP bundle
  - PPP multilink member-interface—Interface type, interface specifier, and administrative status (up or down) for an MLPPP member link
  - Network interface administrative status—Indicates whether the interface for the MLPPP bundle is administratively enabled (open), meaning that the no ppp shutdown command is operational, or administratively disabled (closed), meaning that the ppp shutdown command is operational
  - Link interface administrative status—Indicates whether the interface for the member link is administratively enabled (open), meaning that the no ppp shutdown command is operational, or administratively disabled (closed), meaning that the ppp shutdown command is operational
  - Configured network protocol—Network protocol configured on the interface
  - Fragmentation and reassembly configuration:
    - Link interface fragmentation—Indicates whether MLPPP fragmentation is enabled or disabled on the link interface
    - Link interface fragment size—MLPPP fragment size, in octets, currently in use on the link interface
    - Link interface reassembly—Indicates whether MLPPP reassembly is enabled or disabled on the link interface
    - Link interface administrative MRRU—Administrative MRRU value, in octets, currently in use on the link interface
  - Baseline status—Indicates whether a statistics baseline has been set
  - Interface statistics:
    - packets—Number of packets received (in) and sent (out) on the interface
    - octets—Number of octets received (in) and sent (out) on the interface
    - errors—Number of errors received (in) and sent (out) on the interface
    - discards—Number of packets discarded on receipt (in) or discarded before they were transmitted (out)

      | Note: For the LCP, IPCP, and OSINLCP negotiated options, the command displays a value of “none” if the option was not negotiated.

  - LCP protocol configuration:
    - max-receive-unit—Controls negotiation of the local MRU option; value can be one of the following:
      - use lower layer—MRU of the layer below PPP defines the MRU to be negotiated
      - disabled—MRU option is not to be negotiated
      - a numeric value—MRU value to be negotiated
    - authentication—Controls negotiation of the local authentication option; value can be one of the following:
      - none—Do not negotiate
      - chap—Negotiate CHAP
      - pap—Negotiate PAP
      - chap/pap—Negotiate CHAP, and if it is rejected, negotiate PAP
      - pap/chap—Negotiate PAP, and if it is rejected, negotiate CHAP
    - magic-number—Controls whether the local magic number is negotiated: enabled (negotiate), or disabled (do not negotiate)
    - magic-number-mismatch—Indicates whether the router is configured to ignore the LCP peer magic number and retain the PPP connection when the peer has not negotiated an LCP magic number: ignore (ignore the peer magic number mismatch and retain the PPP connection), or reject (router terminates the PPP connection if it detects a peer magic number mismatch)
    - keepalive-timer—Rate of LCP echo requests, in seconds
    - restart-timer—Retry frequency during LCP, IPCP, and OSINLCP negotiations, in seconds
    - max-terminate—Maximum number of terminate requests
    - max-configure—Maximum number of configure requests
    - max-failure—Maximum number of configure NAKs
  - LCP protocol status:
    - link-status—Indicates the overall status of LCP negotiations, including the following states: initial (idle), starting (ready to negotiate), authenticate (authenticating), and network (LCP is up)
  - LCP negotiated options:
    - max-receive-unit—Negotiated maximum receive unit, in octets, for the local and remote (peer) side of the link
    - max-receive-reconstructed-unit—Negotiated maximum receive reconstructed unit, in octets, for the local and remote (peer) side of the link
    - authentication—Negotiated authentication method (none, pap, or chap) for the local and remote (peer) side of the link
    - magic-number—Negotiated magic number for the local and remote (peer) side of the link
    - pfc—Negotiated pfc (none or enabled) for the local and remote (peer) side of the link
    - acfc—Negotiated acfc (none or enabled) for the local and remote (peer) side of the link

      | Note: The command displays a value of “none” for any negotiated option parameters if the option was not negotiated.

  - LCP Endpoint Discriminator options:
    - local discriminator class—Endpoint discriminator type, format, and address space for the local system
    - local endpoint discriminator—Endpoint discriminator value for the local system within the specified class
    - peer discriminator class—Endpoint discriminator type, format, and address space for the remote system
    - peer endpoint discriminator—Endpoint discriminator value for the remote system within the specified class
  - LCP protocol statistics:
    - in-keepalive-requests—Number of received keepalive requests (LCP Echo Request) for the life of the interface (since either system boot or interface creation, whichever is later)
    - out-keepalive-requests—Number of transmitted keepalive requests for the life of interface
    - in-keepalive-replies—Number of received keepalive replies for the life of the interface
    - out-keepalive-replies—Number of transmitted keepalive replies for the life of the interface
    - keepalive-failures—Number of keepalive failures reported on the interface
    - max-renegotiation-terminates—Number of renegotiation terminations for the PPP session
  - IPCP protocol configuration:
    - configured—IPCP is configured on this interface (true or false)
    - administrative-status—IPCP administrative status (open or closed)
    - ip-address—Address to be used for negotiation of local IP address option
    - dns-precedence—Used to resolve conflicts during DNS address negotiation
    - local—Local side takes precedence, and the no ppp peer dns command is operative
    - peer—Remote side takes precedence, and the ppp peer dns command is operative
    - wins-precedence—Used to resolve conflicts during WINS address negotiation
    - ipcp-lockout—Terminates an invalid subscriber entry and prevents additional IPCP negotiations (enabled or disabled)
    - max-negotiations—Maximum number of renegotiation attempts that the router accepts before terminating a PPP session
  - IPCP protocol status:
    - operational-status—IPCP operational status (up, down, not present, or not present no resources)
  - IPCP negotiated options:
    - ip-address—Negotiated IP address for the local and remote (peer) side of the link
    - primary-dns-address—Negotiated primary DNS address for the local and remote (peer) side of the link
    - secondary-dns-address—Negotiated secondary DNS address for the local and remote (peer) side of the link
    - primary-wins-address—Negotiated primary WINS address for the local and remote (peer) side of the link
    - secondary-wins-address—Negotiated secondary WINS address for the local and remote (peer) side of the link

      | Note: The command displays a value of “none” for any negotiated option parameters if the option was not negotiated.

  - OSINLCP protocol configuration:
    - configured—OSINLCP is configured on this interface (true or false)
    - administrative-status—OSINLCP administrative status (open or closed)
  - OSINLCP protocol status:
    - operational-status—OSINLCP operational status (up, down, not present, or not present no resources)
    - terminate-reason—Reason for termination of OSINLCP service
  - OSINLCP negotiated options
    - npdu-alignment—Negotiated NPDU alignment for the local and remote (peer) side of the link
- Example 1—Displays information about the MLPPP member links configured in bundle group1

      host1#show ppp interface mlppp group1 members
      PPP interface mlppp group1 is up
       PPP multilink member-interface serial 2/0:1/1 is up
       PPP multilink member-interface serial 2/0:2/1 is up
       PPP multilink member-interface serial 2/0:3/1 is up

- Example 2—Displays information about all MLPPP member links configured for all bundles

      host1#show ppp interface mlppp members
      PPP interface mlppp group1 is up
       PPP multilink member-interface serial 2/0:1/1 is up
       PPP multilink member-interface serial 2/0:2/1 is up
       PPP multilink member-interface serial 2/0:3/1 is up
      PPP interface mlppp group2 is up
       PPP multilink member-interface serial 2/1:1/1 is up
       PPP multilink member-interface serial 2/1:2/1 is up
       PPP multilink member-interface serial 2/1:3/1 is up
      PPP interface mlppp group3
       No member-interfaces found

- Example 3—Displays information about all MLPPP encapsulated links, regardless of whether the links are members of an MLPPP bundle

      host1#show ppp interface mlppp links
      PPP multilink interface serial 2/0:1/1 is up
      PPP multilink interface serial 2/0:2/1 is up
      PPP multilink interface serial 2/0:3/1 is up
      PPP multilink interface serial 2/1:1/1 is up
      PPP multilink interface serial 2/1:2/1 is up
      PPP multilink interface serial 2/1:3/1 is up

- Example 4—Displays configuration information about MLPPP member links configured in bundle group1

      host1#show ppp interface mlppp group1 config
      PPP interface mlppp group1 is up
      Network interface administrative status is open
      Configured network protocol is IPCP
      PPP multilink member-interface ATM 10/0.10 is up
      Link interface administrative status is open
      Link interface fragmentation is enabled
      Link interface fragment size is 128
      Link interface reassembly is enabled
      Link interface administrative MRRU is 2000
      PPP multilink member-interface ATM 10/0.11 is down (lower layer down)
      Link interface administrative status is closed
      Link interface fragmentation is enabled
      Link interface fragment size is 128
      Link interface reassembly is enabled
      Link interface administrative MRRU is 2000
      PPP multilink member-interface ATM 10/0.12 is down (lower layer down)
      Link interface administrative status is closed
      Link interface fragmentation is enabled
      Link interface fragment size is 128
      Link interface reassembly is enabled
      Link interface administrative MRRU is 2000
      PPP multilink member-interface ATM 10/0.13 is down (lower layer down)
      Link interface administrative status is closed
      Link interface fragmentation is enabled
      Link interface fragment size is 128
      Link interface reassembly is enabled
      Link interface administrative MRRU is 2000
      1 mlppp interfaces found

- Example 5—Displays statistics about all configured MLPPP member links configured in bundle group1

      host1#show ppp interface mlppp group1 statistics
      PPP interface mlppp group1 is up
      PPP multilink member-interface ATM 10/0.10 is up
      No baseline has been set
      Interface statistics              in                   out
         packets                        0                    0
         octets                         170                  690
         errors                         0                    0
         discards                       0                    0
      PPP multilink member-interface ATM 10/0.11 is down (lower layer down)
      No baseline has been set
      Interface statistics              in                   out
         packets                        0                    0
         octets                         50                   0
         errors                         0                    0
         discards                       0                    0
      PPP multilink member-interface ATM 10/0.12 is down (lower layer down)
      No baseline has been set
      Interface statistics              in                   out
         packets                        0                    0
         octets                         50                   0
         errors                         0                    0
         discards                       0                    0
      PPP multilink member-interface ATM 10/0.13 is down (lower layer down)
      No baseline has been set
      Interface statistics              in                   out
         packets                        0                    0
         octets                         50                   0
         errors                         0                    0
         discards                       0                    0
      1 mlppp interfaces found

- Example 6—Displays status information about the specified MLPPP bundle

      host1#show ppp interface mlppp group1 status
      PPP interface mlppp group1 is up
      1 mlppp interfaces found

- Example 7—Shows complete configuration, statistics, and status information about the specified MLPPP bundle

      host1#show ppp interface mlppp group1 full
      PPP interface mlppp group1 is up
      Network interface administrative status is open
      Configured network protocol is IPCP
      IPCP protocol configuration
         configured                     true
         administrative-status          open
         ip-address                     1.2.3.4
         dns-precedence                 local
         wins-precedence                local
         max-negotiations               10
      IPCP protocol status
         operational-status             up
      IPCP negotiated options           local               peer
         ip-address                     1.2.3.4             6.7.8.9
         primary-dns-address            none                none
         secondary-dns-address          none                none
         primary-wins-address           none                none
         secondary-wins-address         none                none
      OSINLCP protocol configuration
         configured                     false
         administrative-status          open
      OSINLCP protocol status
         operational-status             not present

         terminate-reason               not configured
      PPP multilink member-interface serial 2/0:1/1 is up
      Link interface administrative status is open
      No baseline has been set
      Interface statistics              in                  out
         packets                        0                   0
         octets                         1488                1972
         errors                         0                   0
         discards                       0                   0
      LCP protocol configuration
         max-receive-unit               use lower layer
         authentication                 none
         magic-number                   enabled
         magic-number-mismatch          ignore
         keepalive-timer                30 seconds
         restart-timer                  3 seconds
         max-terminate                  2
         max-configure                  10
         max-failure                    5
      LCP protocol status
         link-status                    network

      LCP negotiated options            local               peer
         max-receive-unit               1590                1590
         max-receive-reconstructed-unit 1590                1590
         authentication                 none                none
         magic-number                   0x6c079eb0          0x2c5a5798
         pfc                            none                none
         acfc                           none                none
      LCP Endpoint Discriminator options
         local discriminator class      Locally Assigned Address
         local endpoint discriminator   0x31393933313030303800001b000001
         peer discriminator class       Locally Assigned Address
         peer endpoint discriminator    0x31393933313030303800001b000002
      LCP protocol statistics
         in-keepalive-requests          70
         out-keepalive-requests         70
         in-keepalive-replies           70
         out-keepalive-replies          70
         keepalive-failures             0
         max-renegotiation-terminates   10
      PPP multilink member-interface serial 2/0:2/1 is up
      Link interface administrative status is open
      No baseline has been set
      Interface statistics              in                  out
         packets                        0                   0
         octets                         1508                1996
         errors                         0                   0
         discards                       0                   0
      LCP protocol configuration
         max-receive-unit               use lower layer
         authentication                 none
         magic-number                   enabled
         magic-number-mismatch          ignore
         keepalive-timer                30 seconds
         restart-timer                  3 seconds
         max-terminate                  2
         max-configure                  10
         max-failure                    5
      LCP protocol status
         link-status                    network
      LCP negotiated options            local               peer
         max-receive-unit               1590                1590
         max-receive-reconstructed-unit 1590                1590
         authentication                 none                none
         magic-number                   0x7ada4a05          0x1bb178cd
         pfc                            none                none
         acfc                           none                none

      LCP Endpoint Discriminator options
         local discriminator class      Locally Assigned Address
         local endpoint discriminator   0x31393933313030303800001b000001
         peer discriminator class       Locally Assigned Address
         peer endpoint discriminator    0x31393933313030303800001b000002
      LCP protocol statistics
         in-keepalive-requests          71
         out-keepalive-requests         71
         in-keepalive-replies           71
         out-keepalive-replies          71
         keepalive-failures             0
      PPP multilink member-interface serial 2/0:3/1 is up
      Link interface administrative status is open
      No baseline has been set
      Interface statistics              in                  out
         packets                        0                   0
         octets                         1568                2068
         errors                         0                   0
         discards                       0                   0
      LCP protocol configuration
         max-receive-unit               use lower layer
         authentication                 none
         magic-number                   enabled
         magic-number-mismatch          ignore
         keepalive-timer                30 seconds
         restart-timer                  3 seconds
         max-terminate                  2
         max-configure                  10
         max-failure                    5
      LCP protocol status
         link-status                    network
      LCP negotiated options            local               peer
         max-receive-unit               1590                1590
         max-receive-reconstructed-unit 1590                1590
         authentication                 none                none
         magic-number                   0x31cc52e0          0x32ebdec6
         pfc                            none                none
         acfc                           none                none
      LCP Endpoint Discriminator options
         local discriminator class      Locally Assigned Address
         local endpoint discriminator   0x31393933313030303800001b000001
         peer discriminator class       Locally Assigned Address
         peer endpoint discriminator    0x31393933313030303800001b000002
      LCP protocol statistics
         in-keepalive-requests          74
         out-keepalive-requests         74
         in-keepalive-replies           74
         out-keepalive-replies          74
         keepalive-failures             0
      1 mlppp interfaces found

- Example 8—Displays information about the MLPPP interface

      host1#show ppp interface mlppp 0/0-1 full
      PPP interface mlppp 0/0-1 is up
      Network interface administrative status is open
      Configured network protocols are IPCP, IPV6CP
      IPCP protocol configuration
         configured                     true
         administrative-status          open
         ip-address                     192.168.1.1
         dns-precedence                 local
         wins-precedence                local
         ipcp-netmask-option            disabled
         ipcp-lockout                   enabled
      IPCP protocol status
         operational-status             up
      IPCP negotiated options           local               peer
         ip-address                     192.168.1.1         100.100.100.17
         ip-address-mask                none                none
         primary-dns-address            none                none
         secondary-dns-address          none                none
         primary-wins-address           none                none
         secondary-wins-address         none                none
      IPV6CP protocol configuration
         configured                     true
      ...

      PPP multilink member-interface ATM 0/0.10 is up
      Link interface administrative status is open
      Link interface fragmentation is enabled
      Link interface fragment size is (use MTU)
      Link interface reassembly is enabled
      Link interface administrative MRRU is (use MRU)
      Link interface hash-link-selection is disabled
      No baseline has been set
      ...
      Authentication status
         grant                          true
         session-timeout                31622400 seconds
         inactivity-timeout             none
         monitor-ingress-only           false
         accounting-timeout             none
         peer-ip-address                100.100.100.17
         peer-ip-address-mask           none
         peer-primary-dns-address       none
         peer-secondary-dns-address     none
         peer-primary-wins-address      none
         peer-secondary-wins-address    none
         peer-ipv6-interface-id         none

- See show ppp interface.

show ppp interface summary

- Use to display a summary of all the multilinked and nonmultilinked PPP interfaces configured on the router.
- Field descriptions
  - PPP Status—Non-multilinked PPP interfaces
  - Configuration status—Indicates the configuration state of the PPP interface, IPCP, IPv6CP , OSINLCP, or MPLS
    - configured—Interface or protocol is configured
    - notConfigured—Interface or protocol is not configured
  - Administrative status—Indicates the administrative state of the PPP interface, IPCP, IPv6CP , OSINLCP, or MPLS
    - open—Interface or protocol is administratively enabled
    - closed—Interface or protocol is administratively disabled
  - Operational status (Interface)—Indicates the operational state of the PPP interface
    - up—Interface is operational
    - down—Interface is not operational because of a problem in the PPP layer
    - lowerDown—Interface is not operational because a lower layer in the protocol stack is down
    - notPresent—Interface is not operational because the hardware is unavailable
    - passive—Interface is waiting for the peer to send an LCP confReq message
    - tunnel—Interface is being redirected through a tunnel
  - Operational status (Ip, Ipv6, Osi, Mpls)—Indicates the operational state of the IPCP, IPv6CP, OSINLCP, or MPLS protocol
    - up—Protocol is operational
    - down—Protocol is not operational because of a problem in the PPP layer
    - notPresent—Protocol is not operational because it does not exist
    - noResources—Protocol is not operational because it does not exist due to a lack of resources
  - PPP Multilink Status—Multilinked PPP interfaces
- Example

      host1#show ppp interface summary
      PPP Status
      Configuration status     configured notConfigured
         Interface             4000       n/a
         Ip                    4000       0
         Ipv6                  0          4000
         Osi                   0          4000
         Mpls                  0          4000
      Administrative status    open       closed
         Interface             4000       0
         Ip                    4000       0
         Ipv6                  4000       0
         Osi                   4000       0
         Mpls                  4000       0
      Operational status       up         down       notPresent noResources
         Interface             4000       0          0          n/a
         Ip                    4000       0          0          0
         Ipv6                  0          0          4000       0
         Osi                   0          0          4000       0
         Mpls                  0          0          4000       0
      Operational status       lowerDown  passive    tunnel
         Interface             0          0          0

      PPP Multilink Status
      Configuration status     configured notConfigured
         Link Interface        8000       n/a
         Network Interface     2000       n/a
         Ip                    2000       0
         Ipv6                  0          2000
         Osi                   0          2000
         Mpls                  0          2000
      Administrative status    open       closed
         Link Interface        8000       0
         Network Interface     2000       0
         Ip                    2000       0
         Ipv6                  2000       0
         Osi                   2000       0
         Mpls                  2000       0
      Operational status       up         down       notPresent noResources
         Link Interface        8000       0          0          n/a
         Network Interface     2000       0          0          n/a
         Ip                    2000       0          0          0
         Ipv6                  0          0          2000       0
         Osi                   0          0          2000       0
         Mpls                  0          0          2000       0
      Operational status       lowerDown  passive    tunnel
         Link Interface        0          0          0
         Network Interface     0          0          0

- See show ppp interface summary.