Country/Region

- United States
- ASEAN Region
- Australia
- 中国 - China
- France
- Deutschland - Germany
- India
- Italia - Italy
- 日本 - Japan
- 대한민국 - Korea
- Россия - Russia
- España - Spain
- 台灣 - Taiwan
- United Kingdom

Contact Us
|
Country/Region
United States

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

# scramble

#### Syntax

[ no ] scramble

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Enables cell scrambling on a T3 Frame interface. The no version disables cell scrambling on the interface. If you issue this command, be sure to issue the dsu mode and dsu bandwidth commands. Otherwise, the interface may drop packets unexpectedly.

#### Mode

Controller Configuration

#### Published: 2010-10-19

Help
|
My Account
|
Log Out