Country/Region

- United States
- ASEAN Region
- Australia
- 中国 - China
- France
- Deutschland - Germany
- India
- Italia - Italy
- 日本 - Japan
- 대한민국 - Korea
- Россия - Russia
- España - Spain
- 台灣 - Taiwan
- United Kingdom

Contact Us
|
Country/Region
United States

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

# show atm vc atm

#### Syntax

show atm vc { description | atm interfaceSpecifier { vcd | vpi-vci vpi vci } } [ delta ] [ filter ]

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Displays OAM statistics on a VC. You can specify the circuit to display by entering the VCD, or by using the vpi-vci keyword and specifying the VPI and VCI. You can also specify the circuit to display by entering the description configured for the ATM 1483 subinterface on which the VC resides.

#### Options

- description—Text string or alias assigned to the ATM 1483 subinterface (with the atm atm1483 description command) on which the VC resides; up to 255 characters
- interfaceSpecifier—Particular interface; format varies according to interface type; see Interface Types and Specifiers
- vcd—VCD identifying the VC
- vpi—Virtual path identifier
- vci—Virtual circuit identifier
- delta—Displays baselined statistics
- filter—See Filtering show Commands

#### Mode

Privileged Exec, User Exec

#### Published: 2010-10-19

Help
|
My Account
|
Log Out