Country/Region

- United States
- ASEAN Region
- Australia
- 中国 - China
- France
- Deutschland - Germany
- India
- Italia - Italy
- 日本 - Japan
- 대한민국 - Korea
- Россия - Russia
- España - Spain
- 台灣 - Taiwan
- United Kingdom

Contact Us
|
Country/Region
United States

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

## Related Documentation

- For a list of shared shaper terms, see Shared Shaping Overview
- Configuring Compound Shared Shaping

# Compound Shared Shaping Overview

Compound shared shaping is a hardware-assisted mode that can control bandwidth for all scheduler objects associated with the subscriber logical interface. Thus it can manage voice and video queues in addition to data queues, so that the shared rate cannot be exceeded.

Compound shared shaping responds to changes in traffic rates more rapidly than simple shared shaping, in the order of milliseconds.

## Supported Hardware for Compound Shared Shaping

You can configure compound shared shaping on a line module with the EFA2 or TFA hardware.

The EFA2 implementation is different from the EFA ASIC, which does not implement compound shared shaping. Issue the show qos shared-shaper command to determine whether compound shared shapers are supported for the line module. Contact your Juniper Networks account representative for more information about line modules with the EFA2 ASIC.

The TFA hardware is only available on the ES2 10G LM on the E120 and E320 Broadband Services Routers.

If you configure a compound shared shaper on hardware that does not support it, the CLI displays the following message:

host1config)#ERROR 02/08/2005 14:06:36 qos: line card in slot 11: EFA2 hardware not installed. 1 compound shared shaper(s) converted to simple.

QoS automatically converts the compound shared shaper to a simple shared shaper.

| Note: Compound shared shaping is not supported by the frame forwarding ASIC (FFA).

## Bandwidth Allocation for Compound Shared Shaping

The compound shared-shaper mechanism actively allocates the bandwidth it receives from the hierarchical scheduler to each active constituent, based on its own rules, independent of the hierarchical scheduler. Constituents are either priority constituents or weighted constituents. These attributes are specified using the shared-shaper-constituent command.

Compound shared-shaper scheduling allocates bandwidth as follows:

1. Priority constituents consume as much of the shared bandwidth as they can, subject to the bandwidth allocated to them by the hierarchical scheduler.
2. Priority constituents are ordered according to their priority.
3. The weighted constituents subdivide the remaining shared bandwidth in proportion to their shared weights, again subject to the bandwidth allocated to them by the hierarchical scheduler.

## Related Documentation

- For a list of shared shaper terms, see Shared Shaping Overview
- Configuring Compound Shared Shaping

#### Published: 2010-09-22

Help
|
My Account
|
Log Out