# ppp multilink multiclass reassembly

#### Syntax

[ no ] ppp multilink multiclass reassembly [ trafficClassName ]*

#### Release Information

Command introduced in JunosE Release 11.1.0.

#### Description

Enables reassembly on a specified multilink class. The maximum received reconstructed unit (MRRU) value of each class is the same as that of the MLPPP link. The no version disables reassembly on all multilink classes, or on the specified multilink classes if you include one or more traffic class names.

#### Options

- trafficClassName—Name of a QoS traffic class. You can enable reassembly for up to eight traffic classes. You must specify the best-effort traffic class in the command or the command fails.
- *—Indicates that one or more parameters can be repeated multiple times in a list in the command line

#### Mode

Interface Configuration, Profile Configuration, Subinterface Configuration

#### Related Documentation

- Configuring Multiclass MLPPP
- Configuring Reassembly on Multiclass MLPPP Interfaces