# Monitoring Subscriber Interfaces Overview

#### Purpose

The state of the subscriber interface is determined by state of the Ethernet interface and the existence of the primary IP interface, which you can monitor with the show ip interface command. For information about using the show ip interface command, see the Monitoring IP section in JunosE IP Services Configuration Guide .

#### Action

You can use the show ip demux interface command to monitor the configuration of subscriber interfaces.