Country/Region

- United States
- ASEAN Region
- Australia
- 中国 - China
- France
- Deutschland - Germany
- India
- Italia - Italy
- 日本 - Japan
- 대한민국 - Korea
- Россия - Russia
- España - Spain
- 台灣 - Taiwan
- United Kingdom

Contact Us
|
Country/Region
United States

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

# show bridge1483 interface

#### Syntax

show bridge1483 interface [ atm interfaceSpecifier ] [ filter ]

To display summary information:

show bridge1483 interface summary

#### Release Information

Command introduced before JunosE Release 7.1.0.
atm keyword and interfaceSpecifier variable added in JunosE Release 7.2.0.

#### Description

Displays configuration and status information for all bridged Ethernet interfaces currently configured on the router. Alternatively, you can use the summary keyword to display only brief summary information for all bridged Ethernet interfaces.

#### Options

- atm—Specifies ATM interfaces
- interfaceSpecifier—Particular interface; format varies according to interface type; see Interface Types and Specifiers
- filter—See Filtering show Commands
- summary—Displays only the total number of bridged Ethernet interfaces currently configured on the router

#### Mode

Privileged Exec, User Exec

#### Published: 2010-10-19

Help
|
My Account
|
Log Out