Country/Region

- United States
- ASEAN Region
- Australia
- 中国 - China
- France
- Deutschland - Germany
- India
- Italia - Italy
- 日本 - Japan
- 대한민국 - Korea
- Россия - Russia
- España - Spain
- 台灣 - Taiwan
- United Kingdom

Contact Us
|
Country/Region
United States

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

# ntp enable

#### Syntax

[ no ] ntp enable

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Enables NTP services on the router and attaches the NTP client to the current virtual router. The no version disables reception of NTP packets on the router and removes the association between NTP and the virtual router. The default setting is disable.

#### Mode

Global Configuration

#### Published: 2010-10-19

Help
|
My Account
|
Log Out