# ip vrrp track

#### Syntax

ip vrrp vrid track objectName [ decrement priorityValue ]

no ip vrrp vrid track objectName

#### Release Information

Command introduced in JunosE Release 7.2.0.

#### Description

Tracks a specified object and changes the priority of that object when the state of the object changes from an up state to a down state. The priority is decremented by the specified value or by the default value (100; when no decrement value is specified). The object priority is restored when the state of the object changes from a down state to an up state. The no version disables any tracking for the object.

#### Options

- vrid—VRID identifier; a number in the range 1–255
- objectName—Name of the object to track
- priorityValue—Priority value of the VRRP router; a number in the range 1–255; default value is 100

#### Mode

Interface Configuration