# default-fields peer

#### Syntax

[ no ] default-fields peer fieldOptions

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Specifies the fields that will appear by default in the output of subsequently issued show ip bgp summary and show bgp ipv6 summary commands. The no version removes the fields from the output.

#### Options

- fieldOptions—Field(s) to be displayed, in the format
  all | [ dynamic | intro | last-reset-reason | messages-received | messages-sent | more-in-queue | peer-type | prefixes-received | remote-as | rib-version |
  send-queue-length| state | times-up | up-down-time | updates-received | updates-sent ]*
  - all—All available information; not recommended, because this information for each network does not fit on a single line and is difficult to read
  - dynamic—Nature of peer, dynamic or not
  - intro—Introductory information about the state of various BGP attributes; this information is displayed only if you specify this keyword
  - last-reset-reason —Reason for most recent reset
  - messages-received—Total number of messages received from the peer
  - messages-sent—Total number of messages sent to the peer
  - more-in-queue—Status indicating whether any messages are waiting to be sent to this peer
  - peer-type—Type of BGP peer: internal, external, or confederation
  - prefixes-received—Number of unique prefixes received from the peer
  - remote-as—Remote AS number of the peer
  - rib-version—Last RIB version queued to be sent to this peer
  - send-queue-length—Number of messages queued to be sent to this peer
  - state—State of the BGP session
  - times-up—Number of times the session has been established
  - up-down-time—How long the session has been up or down
  - updates-received—Number of update messages received from the peer
  - updates-sent—Number of update messages sent to the peer
  - *—Indicates that one or more parameters can be repeated multiple times in a list in the command line

#### Mode

Router Configuration