Country/Region

- United States
- ASEAN Region
- Australia
- 中国 - China
- France
- Deutschland - Germany
- India
- Italia - Italy
- 日本 - Japan
- 대한민국 - Korea
- Россия - Russia
- España - Spain
- 台灣 - Taiwan
- United Kingdom

Contact Us
|
Country/Region
United States

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

# nas-port-type ethernet

#### Syntax

nas-port-type ethernet { cable | wireless-80211 | wireless-cdma | wireless-umts |
wireless-1x-ev | wireless-other | iapp | value }

no nas-port-type ethernet

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Specifies the RADIUS NAS-Port-Type attribute (61) used for Ethernet interfaces. The no version removes the NAS-Port-Type setting.

#### Options

- cable—Cable
- wireless-80211—Wireless 802.11
- wireless-cdma—Wireless code division multiple access (CDMA)
- wireless-umts—Wireless universal mobile telecommunications system (UMTS)
- wireless-1x-ev—Wireless 1xEV
- wireless-other—Wireless other
- iapp—Inter Access Point Protocol (IAPP)
- value—Number in the range 0–65535

#### Mode

AAA Profile Configuration

#### Published: 2010-10-19

Help
|
My Account
|
Log Out