Country/Region

- United States
- ASEAN Region
- Australia
- 中国 - China
- France
- Deutschland - Germany
- India
- Italia - Italy
- 日本 - Japan
- 대한민국 - Korea
- Россия - Russia
- España - Spain
- 台灣 - Taiwan
- United Kingdom

Contact Us
|
Country/Region
United States

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

## Related Documentation

- Policy Rule Precedence

# user-packet-class

#### Syntax

[ no ] [ suspend ] user-packet-class userPacketClassValue

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Adds a user packet class rule to a policy list that sets the user packet class attribute of packets that match the current classifier control list. The no version removes a user packet class from a policy list; the suspend version temporarily suspends the policy rule; the no suspend version resumes application of a suspended rule.

| Note: This command replaces the Policy List Configuration version of the user-packet-class command, which may be removed completely in a future release.

#### Options

- userPacketClassValue—User packet class value assigned to packets, in the range 0–15

#### Mode

Classifier Group Configuration

## Related Documentation

- Policy Rule Precedence

#### Published: 2010-10-19

Help
|
My Account
|
Log Out