# Monitoring RADIUS Override Settings

#### Purpose

Display the current RADIUS override settings.

#### Action

To display the RADIUS override settings:

    host1:vrXyz7#show radius override
    nas-ip-addr: nas-ip-addr
    nas-info:    from authentication virtual router

#### Meaning

Table 27 lists the show radius override command output fields.

Table 27: show radius override Output Fields

Field Name | Field Description
--- | ---
nas-ip-addr | Either the NAS-IP-Address [4] attribute is used, or it is overridden with the Tunnel-Client-Endpoint [66] attribute.
nas-info | Either the NAS-IP-Address [4] and NAS-Identifier [32] attributes of the virtual router generating the accounting information are used, or they are overridden with the respective attributes of the authentication virtual router.

#### Related Documentation

- show radius override