Country/Region

- United States
- ASEAN Region
- Australia
- 中国 - China
- France
- Deutschland - Germany
- India
- Italia - Italy
- 日本 - Japan
- 대한민국 - Korea
- Россия - Russia
- España - Spain
- 台灣 - Taiwan
- United Kingdom

Contact Us
|
Country/Region
United States

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

## Related Documentation

- Monitoring LDP-Related Settings for VPLS in the JunosE BGP and MPLS Configuration Guide

# show ldp vpls

#### Syntax

show [ mpls ] ldp vpls [ vplsName | neighbor ipAddress ] [ filter ]

#### Release Information

Command introduced in JunosE Release 8.2.0.

#### Description

Displays MPLS configuration information for a VPLS instance that uses LDP as the signaling protocol. You can display information for a specific VPLS instance, for a specific neighbor address, or for all VPLS instances configured on the router.

#### Options

- mpls—Specifies optional keyword for compatibility with non–E Series implementations
- vplsName—Name of a VPLS instance created with the bridge vpls transport-virtual-router command
- ipAddress—IP address of a neighbor in the VPLS domain
- filter—See Filtering show Commands

#### Mode

Privileged Exec, User Exec

## Related Documentation

- Monitoring LDP-Related Settings for VPLS in the JunosE BGP and MPLS Configuration Guide

#### Published: 2010-10-19

Help
|
My Account
|
Log Out