# Index

Symbols A B C D E F G H I J L M N O P Q R S T U V W X

Symbols

> 10-Gbps SRP module
> 10/100Base-T port 1, 2, 3
> –48 VDC

A

> access line modules
> access, management
>   setting up console 1, 2
>   SNMP 1, 2
>   Telnet setup
> accessing fan tray
> agency certification 1, 2, 3, 4
> air filter
>   replacing
> airflow
>   rack-mounted installation and
>   specifications 1, 2, 3
> alarm ports
> amperage 1, 2, 3
> antistatic bags and containers
> assembly numbers, locating
> assigning an IP address

B

> BNC connector 1, 2
> booting
>   LED activity

C

> cable-management bracket
>   installing
> cables
>   failure
>   I/O modules
>   pinouts
>   power input module
>   recommendations
>   redundant port
>   required
>   SRP I/O modules 1, 2
> cabling
>   ERX routers
>   HSSI connectors
>   RJ-45 connectors 1, 2
>   SC duplex connectors 1, 2
>   SRP I/O modules 1, 2
>   X.21/V.35 connectors
> Case Manager
> certifications 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 12
> circulation, air
> classification, packet
> cleaning
> CLI (command-line interface)
> clock source input ports
> clocking problems
> color code, power cable
> combinations of line modules
> command-line interface
> compliance
>   product reclamation and recycling
>   requirements 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 12
> components
>   returning
>   storing
> configuring cables 1, 2
> configuring management access
> configuring Telnet
> connecting console to router
> connectors, pinouts
> console
>   for management access 1, 2
>   ports
>     RS-232 1, 2
> consumption, power 1, 2, 3, 4
> conventions
>   notice icons
>   text and syntax
> current (electrical) requirements 1, 2, 3
> customer support
>   contacting JTAC

D

> DB-9 connector 1, 2, 3, 4, 5
> DC power 1, 2
> detecting double-bit error
> Device Management System, NMC-RX
> diagnosing problems
> diagnostic LEDs
> dimensions of ERX routers 1, 2, 3
> dissipation, heat 1, 2, 3
> distribution rack
> documentation set
>   comments on
> double-bit errors
>   detecting
>   troubleshooting

E

> EIA distribution rack
> ejectors, module
> electrical requirements 1, 2, 3, 4
> electronic equipment, recycling
> environmental requirements
> ERX14xx models
>   fan tray
>   front view
>   rear view
> ERX310 Broadband Services Router
>   front view
>   power cord warnings
>   rear view (AC model)
>   rear view (DC model)
> ERX310 router
>   fan tray
> ERX705 router
> ERX7xx models
>   fan tray
>   front view
>   rear view
>   slot identification and grouping
> ESD (electrostatic discharge)
> ESD grounding jack, chassis
> Ethernet link
> external timing ports
> E Series routers
>   assigning IP address to
>   cabling
>   cabling recommendations
>   dimensions 1, 2, 3
>   electrical requirements 1, 2, 3
>   hardware
>   installing 1, 2
>   installing components
>   installing modules
>   lifting 1, 2
>   maintenance
>   management access 1, 2
>   models
>   modules
>   power requirements 1, 2, 3
>   powering down
>   powering up
>   safety guidelines 1, 2, 3
>   site planning
>   slot groups and identification
>   space requirements
>   troubleshooting 1, 2

F

> failure, fan
> failures
> FAN FAIL LED
> FAN OK LED
> fan tray
>   hot-swapping
> fans
>   failure 1, 2
>   installing
>   location
>   redundancy
>   removing
>   status
> far-end receive failure
> FERF (far end receive failure)
> filler panel
> filter, air
> Flash cards
> flow, air

G

> grounding jack, ESD

H

> halt command 1, 2
> hardware
>   cable configuration 1, 2
>   reclamation and recycling
>   redundancy features
>   repairing and replacing
> hazardous materials, reclamation and recycling
> heat dissipation 1, 2, 3, 4
> high-availability mode
> hot-swapping
>   fan trays
>   modules
> HSSI connectors, cabling
> humidity requirements 1, 2, 3
> HyperTerminal

I

> I/O modules
>   cables
>   installing
>   installing redundancy
>   OC48 Frame APS
>   removing
>   SFPs
>   SRP
> installing ERX routers
>   site planning
> installing modules
>   I/O modules
>   line modules
>   order of installation
>   slot groups and module arrangements
>   SRP I/O modules
>   SRP modules
> installing NVS cards 1, 2
> installing redundancy I/O modules
> installing redundancy midplane
> installing SFPs
> installing spare line modules
> IP address, assigning

J

> JTAC, contacting

L

> lead in equipment, reclamation and recycling
> LEDs
>   abnormal activity
>   fans
>   line modules
>   normal activity
>   redundancy status
>   SRP modules 1, 2
> lifting router
> line modules
>   access
>   combinations
>   installing
>   installing spare
>   LEDs 1, 2
>   OC48
>   performance rate
>   redundancy 1, 2
>   removing
>   slot groups
>   uplink
> location, for ERX routers

M

> maintenance, system
> management access
>   setting up console 1, 2
>   SNMP 1, 2
>   Telnet setup
> Management Information Bases
> management port
>   10/100Base-T 1, 2
> managing modules
> manuals
>   comments on
> mechanical requirements for distribution rack
> memory, upgrading
> MIBs (Management Information Bases)
> midplane
>   redundancy
> models
>   ERX router
> module reset button
> modules
>   failure
>   hot-swapping
>   installing
>     order of installation
>   managing
>   removing
>   repairing and replacing
>   replacing
>   self-testing
>   storing
>   types of
> monitoring LEDs
> monitoring temperature
> mounting kits
> mounting posts for rack

N

> network management
>   setting up console 1, 2
>   SNMP 1, 2
>   Telnet setup
> NMC-RX Device Management System
> notice icons
> NVS cards
>   installing 1, 2
>   storing

O

> OC48 modules
> ONLINE LED
> order of module installation

P

> packaging, recycling
> packet classification
> packing instructions
> PCMCIA slot, SRP modules
> performance rate, line modules
> PIM
>   replacing
> pinouts, router cables and connectors
> planning site for installation
> plenum
> ports
>   alarm
>   external timing
>   management
>   redundancy 1, 2
>   status LEDs
> power
>   cabling power input module 1, 2
>   consumption
>     system 1, 2, 3, 4
>   dissipation 1, 2, 3
>   failures 1, 2
>   redundancy
>   source A
>   source B
>   specifications 1, 2, 3, 4
> power cord warnings
> power input module
>   cabling
>   replacing
> power requirements 1, 2, 3
> power switches 1, 2
> powering down router
> powering up router
> preinstallation responsibilities
> preparing site for installation
> primary SRP module
> problems
> product numbers, locating

Q

> QoS, packet classification for

R

> rack, distribution
> reclamation and recycling
> recycling Juniper Networks equipment
> redundancy
>   line module status
>   midplane
>   SRP modules
>   status
> redundancy features (hardware)
>   fans
>   line modules
>   ports 1, 2
>   SRP modules
> redundancy midplane
>   installing
> REDUNDANT LED
> release mechanisms for SFPs
> removing components
> removing modules
> removing SFPs
> repacking components
> repairing hardware components
> replacing components
> replacing modules
> replacing NVS cards 1, 2
> replacing SFPs 1, 2
> reset button, module
> Restriction of Hazardous Substances (RoHS) Directive, recycling equipment
> Return Materials Authorization
> returning product
> RJ-45 connectors, cabling 1, 2
> RMA
> RoHS (Restriction of Hazardous Substances) Directive, recycling equipment
> RS-232 port 1, 2, 3, 4

S

> safety
>   agency certification 1, 2, 3
>   guidelines 1, 2, 3
> SC duplex connectors, cabling 1, 2
> self-testing, modules
> serial numbers, locating
> SFPs (small form-factor pluggable transceivers)
>   installing
>   removing
>   storing
> show configuration command
> show environment command 1, 2
> show hardware command
> show version command 1, 2
> show interface gigabitEthernet command
> site planning
> size
>   of ERX routers 1, 2, 3
>   of rack
> slot disable command
> slot groups
>   ERX1410 router
>   ERX7xx models
>   overloading
> small form-factor pluggable transceivers
> SMB connectors
> SNMP for management access 1, 2
> SODIMMs
> software
>   configuration
>   upgrading
> space requirements 1, 2, 3, 4, 5
> spare line modules, installing
> specifications
>   airflow 1, 2, 3
>   dimensions 1, 2, 3
>   distribution rack
>   electrical 1, 2, 3, 4
>   heat dissipation 1, 2, 3
>   space 1, 2, 3
>   weight 1, 2, 3
> SRP I/O modules
>   cabling 1, 2
>   installing
>   removing
> SRP modules
>   errors on
>   installing
>   LEDs on 1, 2
>   models
>   PCMCIA slot
>   powering down
>   redundancy 1, 2
>   removing 1, 2
> standby SRP module
> starting ERX routers
> status, redundancy
> storing, modules and components
> support, technical, See technical support
> switches, power 1, 2
> switching on router
> switchover to spare line module
> synchronize command
> system maintenance

T

> technical support
>   contacting JTAC
> Telnet connection to router
> temperature
>   excessive 1, 2
>   monitoring
>   requirements 1, 2
> text and syntax conventions
> thermal protection mode 1, 2, 3
> timing inputs, external 1, 2
> tools needed 1, 2, 3, 4, 5
> troubleshooting
>   booting
>   cables 1, 2
>   clocking
>   double-bit errors
>   Ethernet link
>   fans 1, 2
>   FERF
>   LED activity for
>   modules 1, 2
>   power failure 1, 2
>   safety guidelines 1, 2

U

> uninstalling modules
> upgrading software
> uplink line modules

V

> ventilation
> voltage requirements 1, 2, 3

W

> warnings, safety
> Waste Electrical and Electronic Equipment (WEEE) Directive., See WEEE Directive
> WEEE (Waste Electrical and Electronic Equipment) Directive, recycling equipment
> weight
>   of ERX routers 1, 2, 3
>   of rack 1, 2
> wrist strap, antistatic

X

> X.21/V.35 connectors, cabling