# slot replace

#### Syntax

slot replace slotNum

#### Release Information

Command introduced in JunosE Release 9.1.0.

#### Description

Enables you to replace an ES2 4G LM or an ES2 10G LM with a different type of module without erasing the interface configuration on the slot. You can use this command to replace these line modules if they both are paired with the ES2-S1 GE-8 IOA or the ES2-S1 Redund IOA installed. Issue this command after you install the new type of line module in the slot. There is no no version.

#### Options

- slotNum—Number of the selected slot in the router; for the E120 router, a number in the range 0–5; for the E320 router, a number in the range 0–5 or 11–16

#### Mode

Global Configuration