# ip igmp last-member-query-interval

#### Syntax

ip igmp last-member-query-interval tenthsOfaSecond

no ip igmp last-member-query-interval

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Specifies in tenths of a second the maximum time the router waits for a response after sending a last member query. The router sends a last member query when it receives an IGMPv2 leave message or an IGMPv3 state change report. The no version restores the default value, 10 tenths of a second (1 second).

#### Options

- tenthsOfaSecond—Time interval between receipt of an IGMP leave message and sending out of a query in the range 1–254 tenths of a second. Using a lower value allows members to leave groups more quickly.

#### Mode

Interface Configuration, Profile Configuration