# ip source-route

#### Syntax

[ no ] ip source-route [ vrf vrfName ]

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Enables the forwarding of source-routed packets in a VR or VRF. The no version disables forwarding. Forwarding is disabled by default in all VRs.

#### Options

- vrfName—Name of the VRF; string of 1–32 alphanumeric characters

#### Mode

Global Configuration