# show resource

#### Syntax

show resource [ [ if-type { atm-active-sub-if | atm-sub-if | atm-vc | ip | ppp-link }
[ system | slot slot ] ] | [ threshold [ trap [ status ] ] ]

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Displays statistical information about resources and their current threshold configurations.

#### Options

- if-type—Indicates interface type; see Interface Types and Specifiers
- atm-active-sub-if—Active ATM subinterfaces
- atm-sub-if—Both active and inactive ATM subinterfaces
- atm-vc—ATM virtual circuits
- ip—IP interfaces
- ppp-link—PPP link interfaces
- system—All slots on the system
- slot—Number of the chassis slot in the range 0–2 (ERX310 model), 0–6 (ERX7xx models), and 0–13 (ERX14xx models)
- threshold—Displays threshold information (optional keyword when used alone)
- trap—Displays threshold trap status
- status—Displays threshold trap status (optional keyword)

#### Mode

Privileged Exec