Country/Region

- United States
- ASEAN Region
- Australia
- 中国 - China
- France
- Deutschland - Germany
- India
- Italia - Italy
- 日本 - Japan
- 대한민국 - Korea
- Россия - Russia
- España - Spain
- 台灣 - Taiwan
- United Kingdom

Contact Us
|
Country/Region
United States

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

# net

#### Syntax

[ no ] net networkEntityTitle

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Configures an IS-IS network entity title for the specified routing process. The no version removes a specific NET. You must specify a NET. You can add multiple manual area IDs by adding multiple NETs with the same system ID. The last NET cannot be removed.

#### Options

- networkEntityTitle—NET that specifies the area ID and the system ID for an IS-IS routing process; can be either an address or a name; in the form of: areaID.systemID.nSelector
  For example:
  - areaID—All bytes in front of the system ID; the number of bytes can vary from 1–13 bytes
  - systemID—Always 6 bytes and cannot vary
  - nSelector—Last byte; always 0

#### Mode

Router Configuration

#### Published: 2010-10-19

Help
|
My Account
|
Log Out