Country/Region

- United States
- ASEAN Region
- Australia
- 中国 - China
- France
- Deutschland - Germany
- India
- Italia - Italy
- 日本 - Japan
- 대한민국 - Korea
- Россия - Russia
- España - Spain
- 台灣 - Taiwan
- United Kingdom

Contact Us
|
Country/Region
United States

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

# version

#### Syntax

version { 1 | 2 }

no version

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Specifies the global RIP version. The no version reverts to the default value, RIP version 1. Use the ip rip receive and ip rip send version commands to specify the RIP version for a specific interface.

#### Options

- 1—RIP version 1
- 2—RIP version 2

#### Mode

Address Family Configuration, Router Configuration

#### Published: 2010-10-19

Help
|
My Account
|
Log Out