# mark-user-priority

#### Syntax

[ no ] [ suspend ] mark-user-priority userPriorityValue

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Defines a policy rule that specifies the value of the 802.1p VLAN user priority bits. The no version removes the rule from the policy list; the suspend version temporarily suspends the policy rule; the no suspend version resumes application of a suspended rule.

| Note: This command replaces the Policy List Configuration version of the mark-user-priority command, which may be removed completely in a future release.

#### Options

- userPriorityValue—EXP bit value assigned to packets; number in the range 0–7

#### Mode

Classifier List Configuration

#### Related Documentation

- Policy Rule Precedence