Country/Region

- United States
- ASEAN Region
- Australia
- 中国 - China
- France
- Deutschland - Germany
- India
- Italia - Italy
- 日本 - Japan
- 대한민국 - Korea
- Россия - Russia
- España - Spain
- 台灣 - Taiwan
- United Kingdom

Contact Us
|
Country/Region
United States

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

## Related Documentation

- Enabling Multiclass MLPPP
- Configuring Multiclass MLPPP

# ppp multilink multiclass

#### Syntax

ppp multilink multiclass [ multilink-classes classNumber ]

no ppp multilink multiclass [ multilink-classes ]

#### Release Information

Command introduced in JunosE Release 11.1.0.

#### Description

Enables multiclass MLPPP on the router, and optionally creates a specified number of multilink classes. The no version without the multilink-classes keyword disables multiclass MLPPP on the router. The no version with the multilink-classes keyword restores the number of multilink classes to the default value, 1.

#### Options

- classNumber—Number of multilink classes that can be created in the range 1–8, with a default value of 1.

#### Mode

Interface Configuration, Profile Configuration, Subinterface Configuration

## Related Documentation

- Enabling Multiclass MLPPP
- Configuring Multiclass MLPPP

#### Published: 2010-10-19

Help
|
My Account
|
Log Out