Country/Region

- United States
- ASEAN Region
- Australia
- 中国 - China
- France
- Deutschland - Germany
- India
- Italia - Italy
- 日本 - Japan
- 대한민국 - Korea
- Россия - Russia
- España - Spain
- 台灣 - Taiwan
- United Kingdom

Contact Us
|
Country/Region
United States

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

# redundancy force-switchover

#### Syntax

redundancy force-switchover { slotNumber | srp }

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Forces the router to switch from the primary line module in the specified slot or the primary SRP module to the spare line module or SRP module. This command overrides the redundancy lockout command. With the srp option, the command is equivalent to the srp switch command. There is no no version.

| Note: This command replaces the redundancy force-failover command, which has been deprecated.

#### Options

- slotNumber—Number of the slot in which the primary line module resides
- srp—Indicates that the router should switch from the active to the standby SRP module

#### Mode

Privileged Exec

#### Published: 2010-10-19

Help
|
My Account
|
Log Out